settingseditor

### ChryslerSettings

When this registry entry is set to TRUE (1), functionality specific to etools is used. This functionality does the following:

- If a feature’s thickness in PC-DMIS is zero and it is non-zero in the Inspection Plan, PC-DMIS assumes that the zero value is because of importing from PC-DMIS 3.5, and it automatically changes the thickness of the feature in the measurement routine.

- When deleting a command in the Change Manager, if there’s a comment with the name [feature_name]_COMMENT, PC-DMIS deletes it as well.

- When importing a feature through the Change Manager, if the feature has a feature locator text defined, PC-DMIS creates a comment with that text and adds it together with the feature.

Entry Name: ChryslerSettings

Entry Type: Whole Number to specify TRUE (1) or FALSE (0). The default value is 0.