laser

#### Filter Type: Weighted Average

This type is only available for Perceptron sensors.

Weighted Average Filter Type

The Weighted Average filter smooths stripe data by computing a new location for each pixel. For each pixel in the stripe, this filter will use a weighted average of its neighboring pixels to compute a new location. This is the default filter.

Neighbor #: This value determines the number of total pixels considered when calculating a new location of any given pixel in a single stripe.

Set Weights: This button sets the relative importance of a given pixel’s neighbor.

Use the up and down arrows for each of the pixel locations. Click OK to save your changes or Cancel to close without saving.

Point Reduction Filter: This check box determines whether or not PC-DMIS filters points along the scan line. If marked, you can select the desired percentage of total points to filter. If cleared, the complete data set is acquired without any filtering.

Example of Point Filtering Disabled

Example of Point Filtering of 50%