miim

### TempComp-202 Gradient temperature limit exceeded

Temperature compensation has been requested but the difference in temperature between a pair or thermistors indicates a temperature gradient that exceeds the configured system limits. Temperature compensation is active but system conditions may preclude achieving the desired system accuracy. The message includes the thermistor numbers and recorded temperatures that caused the warning.

For more information, see "TempComp Error Codes".

What you should do:

1. If possible, correct the identified problem.

2. If the error cannot be explained by the environmental conditions and if the error reoccurs:

You should contact your Giddings & Lewis service representative.