settingseditor

### DccEdgeInitHits

Specifies the default Initial Hits value that will be used in the creation of Edge Points. Initial hits are used to measure the plane around the nominal point location for the Edge Point feature. Initial sample hits are taken only on the initial measurement of the feature during execution of the measurement routine.

Entry Name: DccEdgeInitHits

Entry Type: Whole Number to specify the number of initial hits. The default value is 5.