core

Step 3 - Define the Number of Ports

The final step prior to the actual calibration of the TP200 Probe Changer is to define the number of ports on the rack you are calibrating.

To define the number of ports:

1. Select the Ports tab in the Probe Changer dialog box (Edit | Preferences | Probe Changer):

Probe Changer dialog box - Ports tab

2. In the Active probe changer list, select TYPE=TP200.

3. In the Number of ports box, type the number of ports that you want to define.

4. Click Apply to store this parameter.

The next step starts the calibration process.