miim

## Interfaces

Arduino (Quonset Point)

PC-DMIS should install the required Arduino drivers when you install Notification Center.

To ensure that the Arduino UNO appears as a COM port:

1. Open Device Manager.

2. Ensure that the Arduino UNO appears as a COM port.

3. Test the connection. For details, see "Testing the Lights in a Terminal".

Bluetooth BT6Out (Torino)

To use the Bluetooth BT6Out system:

1. Install the drivers for the USB Bluetooth wireless adapter that is connected to the computer.

2. Pair the Bluetooth BT6Out device. If a communication problem occurs, see "Pairing a BT6OUT Device".

3. Test the connection. For details, see "Testing the Lights in a Terminal".