laser

## Pointcloud Operators

The Pointcloud operator commands listed below perform different operations on cloud of points (COP) commands and other pointcloud operator commands. The units for these commands are defined by the measurement routine.

Versions earlier than PC-DMIS 2014 used a COPOPER keyword prior to the operator command. This COPOPER command is no longer available, and the commands now use a COP prefix. For example, the Filter operator is now COPFILTER.

You can add pointcloud operator commands into your measurement routine in any of these ways:

- Select the Insert | Pointcloud | Operator menu item.

- Select menu items from the following submenus:

- File | Import | Pointcloud - Import from data files to a COP.

- File | Export | Pointcloud - Export to data files from a COP.

- Insert | Pointcloud - Add basic pointcloud commands from this submenu. These include COP and specific point cloud operator commands (Cross Section, Surface Colormap, or Point Colormap) that alter the display of pointclouds in the Graphic Display window.

- Operation | Pointcloud - Alter the number of points that are included in COP commands. Items included in this submenu are: Clean, Empty, Filter, Purge, Reset, and Select.

- Manually type pointcloud operator command into the Edit window. If the cursor is on the command in the Edit window, and you press F9, the Pointcloud Operator dialog box opens.

- From the Pointcloud toolbar, click the appropriate Pointcloud Operator button to open the associated Pointcloud Operator dialog box. The pointcloud operator is applied to the COP.

You must be licensed with the COP option to use Pointcloud operator commands. You cannot use these commands if you are only licensed with the Vision option. Vision should be disabled when using Laser.

More:

Manipulating Pointcloud Operators

Edit the Color Scale

SELECT

CROSS SECTION

SURFACE COLORMAP

POINT COLORMAP

CLEAN

PURGE

FILTER

Pointcloud EXPORT

RESET

EMPTY

Pointcloud IMPORT

BOOLEAN