nc

### Step 2: Install PC-DMIS NC and Define a Machine

1. If you are using a portlock, insert it into your computer or ensure your LMS license is configured for PC-DMIS NC. Your portlock or LMS license should already be programmed to enable the PC-DMIS NC functionality. The CNC licensing options include:

- CNC Licenses - Specifies the number of CNC machines that are connected for use with PC-DMIS.

- NCi - Authorizes the use of PC-DMIS NC interactive instead of the standard PC-DMIS configuration. See "PC-DMIS NCI".

2. Install PC-DMIS.

3. Install the NC Gateway server application.

4. Start NC Gateway.

5. Use NC Gateway to define a test machine. Give the test machine the name of "Test". For information on how to do this, consult the NC Gateway documentation.

6. Close NC Gateway.

Next Step...