miim

#### ZEISS.DLL 2.005n Adds a pair of new configuration options

CHECK_MOVE_POSITION=1

CHECK_MOVE_POSITION_DISTANCE=500

After move command (G02) was sent to the controller it is polled for scales to determine whether the target was achieved (the option is intended for WAIT_OPTIMIZATION=1 mode but can be used separately).

The distance from the target can be set with CHECK_MOVE_POSITION_DISTANCE. The unit is microns; default is 1000 um = 1mm.