Collapse All Expand All

PC-DMIS 2019 R1 Object Library |
TempComp Object Members
See Also Overview Send Topic Feedback | See Object Hierarchy Chart

PCDLRN ActiveX DLL : TempComp Object

Glossary Item Box

# Public Methods

GetOrigin | Gets the reference origin
SetOrigin | Sets the reference origin

# Public Properties

HighThreshold | Double value representing the high temperature threshold.
LowTheshold | Double value representing the low temperature threshold.
MaterialCoefficient | Double value indicating the material coefficient.
RefTemp | Double value representing the reference temperature.
Sensors | String value representing the list of sensors--by number--to be used for temperature compensation. The format of the list is a series of consecutive sensor numbers. The series are specified using the hyphen between the first number and the last number of the series. Each non-consecutive sensor or group of sensors is separated by the comma (or the typical separator for the given locale).

# See Also

TempComp Object

Copyright © 2019. Hexagon Manufacturing Intelligence – Metrology Software, Inc. All Rights Reserved.