Collapse All Expand All

PC-DMIS 2019 R1 Object Library |
SetBoundaryPoint Method
See Also Send Topic Feedback | See Object Hierarchy Chart

index
  Required Long which indicates which boundary point to set.

X
  Required Long that indicates the X value of the boundary point.

Y
  Required Long that indicates the Y value of the boundary point.

Z
  Required Long that indicates the Z value of the boundary point.

PCDLRN ActiveX DLL > BasicScan Object : SetBoundaryPoint Method

Glossary Item Box

# Description

Sets a boundary point.

# Syntax

Visual Basic
    Public Function SetBoundaryPoint( _
       ByVal index As Long, _
       ByVal X As Double, _
       ByVal Y As Double, _
       ByVal Z As Double _
    ) As Boolean

# Parameters

index
  Required Long which indicates which boundary point to set.
X
  Required Long that indicates the X value of the boundary point.
Y
  Required Long that indicates the Y value of the boundary point.
Z
  Required Long that indicates the Z value of the boundary point.

# Remarks

This function works with patch scans. Use the BoundaryPointCount property to set the number of boundary points.

# See Also

BasicScan Object | BasicScan Members

Copyright © 2019. Hexagon Manufacturing Intelligence – Metrology Software, Inc. All Rights Reserved.