core

## Compensating for Temperature

Temperature Compensation Setup dialog box

To open the Temperature Compensation Setup dialog box, select Edit | Preferences | Temperature Compensation Setup.

To set up temperature compensation for your system as shown in this legacy section, you need to start PC-DMIS as an administrator. In addition, the value for the UseTemperatureCompensationV2 registry entry must be False.

This dialog box enables you to compensate for room and part temperature, which increases the accuracy of the inspection process.

To compensate for temperature during multiple arm calibration, see "Using Temperature Compensation with Multiple Arm Calibration" in the "Using Multiple Arm Mode" chapter.

To use advanced options for temperature compensation, see "Using Advanced Temperature Compensation" in the Toolkit Modules documentation. Advanced options enable you to use the continuous temperature compensation ability of the Firmware Distributed Controller (FDC) and Hexagon B3C controller.

More:

Using STP Files

Available Input Parameters

TEMPCOMP Command in the Edit Window

Controller Support

Local Temperature Settings