core

### Auto-Continue Execution

(This item applies to the Comment dialog box, accessible through Insert | Report Command | Comment.)

Auto-continue execution: This check box determines whether or not a comment that PC-DMIS displays during execution closes itself after a specified number of seconds. Operators may find this useful when they use a measuring device that is not near the computer, and they want the execution to continue after a certain amount of time. If you select this check box, the Execution delay (in seconds) box becomes available.

Execution delay (in seconds): This box defines the number of seconds to delay execution while PC-DMIS displays the comment. You can specify any number of seconds from 1 to 600, inclusive.

- If you use an execution delay with a movie file and the movie's play time exceeds the delay value, PC-DMIS waits until the movie finishes playing before continuing.

- If your movie value is shorter than the specified execution delay, the comment displays until the execution delay counts down to zero.

During execution, a count-down timer appears on the Operator comment type's OK button inside parentheses:

For the Yes / No comment type, it appears on the Yes button.

Once the timer reaches zero:

- For an Operator comment, execution continues as if the operator clicked the OK button.

- For a Yes / No comment, execution continues as if the operator clicked the Yes button.