miim

#### CMMAccuracy Options

The registry entries in the CMMAccuracy section in PC-DMIS Settings Editor are:

- Enabled = FALSE - On controllers that have predefined probing parameter sets that you can activate by name with the USEPAR command, set the value to TRUE.

- UseParConfig = DEFAULT - Specifies the name of the parameter set to activate when PC-DMIS first starts. This registry entry is only used if Enabled =TRUE.