settingseditor

### DiagnosticsAutoExport

If you set this registry entry to True, PC-DMIS automatically creates diagnostic files in the root PC-DMIS installation directory each time you execute a measurement routine. The diagnostic files include bitmap images and a descriptive text file with current feature parameters. PC-DMIS overwrites the diagnostic files each time you execute the measurement routine.

The naming convention for the bitmap images is as follows:

<measurement routine name>_<feature ID>_<image number>_of _<total number of feature images><_O or no _O>.BMP

Vision1_PNT1_1_of_1.BMP

Vision1_PNT1_1_of_3_O.BMP

Files with an "_O" at the end of the file name include overlay information.

The naming convention for the text file is as follows:

<measurement routine name>_<feature ID>.DGN

Vision1_PNT1.DGN

Entry Name: DiagnosticsAutoExport

Entry Type: True or False value. The default value is False.