cmm

#### Reset Tips to Theo at Start of Calibration

Reset tips to Theo at start of calibration check box

If you select this check box, the tip or tips undergoing calibration are automatically reset to their original theoretical conditions when the calibration starts. This essentially functions the same as if you had manually clicked the Reset Tips button in the Probe Utilities dialog box before calibration.

This functionality does not apply to all types of operations and all types of hardware, however.

It does not affect a "Qualification Check" operation, because that is only a test of the calibration and does not actually change any calibration related data. It also does not apply when you use infinite wrist devices in a mapped mode.

It is mainly used with the "Calibrate Tips" operation when used with a fixed head, indexing wrist, or infinite wrist if used in an indexing (non-mapped) mode.