miim

### MP-526 RS-232 electronic level interface failure

See the following:

- On an MP-30 system, diagnostics on the MP RS-232 interface board port 1 failed.

The board may have failed or may not be installed in the MP.

- On an SMP system, diagnostics on the electronic level RS-232 interface on the DCC card has failed.

- Diagnostics on the MP RS-232 interface board port 1 failed.

The board may have failed or may not be installed in the MP.

For more information, see "MP Error Codes".

You should contact your Giddings & Lewis service representative.