miim

#### MOVE / MEASURE PARAMETERS

EnableUserParams = TRUE If FALSE, will silently NOT transmit to machine any probing parameter setting part of a PC-DMIS program. That means that the probing will be done with calibration parameters, enforcing technology-free measurement. Moving speeds are still transmitted.

SendSpeedChanges = TRUE If FALSE, will silently NOT transmit to machine move speed changes.

AlwaysSendPrehit = FALSE If TRUE, will force transmission of prehit (and scan retract) distances, regardless of the "EnableUserParams" setting.

AlwaysSendScanSpeed = FALSE If TRUE, will force transmission of scan speed with every scan, regardless of the "EnableUserParams" setting.