core

### Wenzel Interface

The Wenzel interface is used with Wenzel machines with a Wenzel 2010 controller (Native Wenzel Protocol). This interface just requires a single RS232 comm port; no machine parameter file is needed from the original system.

Before you start PC-DMIS, rename the wenzel.dll to interfac.dll.

The Machine Options dialog box (Edit | Preferences | Machine Interface Setup) has these tabs for the Wenzel interface:

Axis tab

See the "Assigning the Machine Axes" topic.

Debug tab

See the "Generating a Debug File" topic.

Additional information for this interface is provided in the Machine Interface Installation Manual (MIIM).

You can access the MIIM help file from this link: .