miim

### Installation Information

Interface DLL - LK.DLL

PCDLRN.INI Section header title - [LK Direct]

Many types of LK controllers use TCP for the controller communication, such as:

- LK-2000-P

- LK4000

- MCC-200

- MCC-300

They all use the same LK.DLL file. The tailored PC-DMIS configuration file handles any differences between the machines. Because of this, these controllers require a Hexagon Manufacturing Intelligence installation.

PC-DMIS needs the original lkcmmdrv.cfg file to establish the parameters for the machine. This file is typically found in C:\ LK\Appdata\CMMCFG. Copy it onto the computer running PC-DMIS. You can find the location of where you should copy the file to in the PC-DMIS configuration file as documented in "Options and Settings".