settingseditor

### DccLineNumHits

Used to define the default value for the Hits option that will be used when a line Auto Feature is created. Defines the number of hits to be used to measure the feature. If the line is bounded, the number of hits specified will be equally spaced between the line's start and end point. If the line is unbounded, the hits are equally spaced along the line's direction vector.

Entry Name: DccLineNumHits

Entry Type: Whole number that specifies the number of permanent hits. The default value is 2.

See the "Working with Contact Path Properties" topic in the PC-DMIS CMM documentation.