Collapse All Expand All

PC-DMIS 2019 R1 Object Library |
PutFeatData Method
See Also Send Topic Feedback | See Object Hierarchy Chart

ID

buffer

dtype

XYZ

IJK

PCDLRN ActiveX DLL > OldBasic Object : PutFeatData Method

Glossary Item Box

# Description

Puts feature data into the command specified by the ID

# Syntax

Visual Basic
    Public Sub PutFeatData( _
       ByVal ID As String, _
       ByVal buffer As FeatData, _
       ByVal dtype As PCDMEASTHEO, _
       ByVal XYZ As XYZTYPES, _
       ByVal IJK As IJKTYPES _
    )

# Parameters

ID
buffer
dtype

  Value | Description
  --- | ---
  PCD__MEAS |
  PCD_THEO |

XYZ

  Value | Description
  --- | ---
  PCD_BALLCENTER |
  PCD_CENTROID |
  PCD_ENDPOINT |
  PCD_MIDPOINT |
  PCD_STARTPOINT |

IJK

  Value | Description
  --- | ---
  PCD__VECTOR |
  PCD_SLOTVECTOR |
  PCD_SURFACEVECTOR |

# Remarks

Parameters, allowed values, and limitations are identical to those of GetFeatData. The data currently in buffer is stored in the feature identified by the ID string.

# See Also

OldBasic Object | OldBasic Members

Copyright © 2019. Hexagon Manufacturing Intelligence – Metrology Software, Inc. All Rights Reserved.