miim

### DCC-1 32 milliseconds since the last D/A update

The digital/analog (D/A) converters on the DCC board have not been updated for at least 32 milliseconds.

For more information, see "DCC Error Codes".

What you should do:

1. To clear the error, power the MP down.

2. Reseat the DCC board.

3. Power the MP back up.

4. If the error reoccurs, contact your Giddings & Lewis service representative.