core

### Supported ISO 14405-1 Modifiers

The Size command supports the following modifiers that are defined in the ISO 14405-1 standard:

- (LP) - Two-point size

- (GG) - Least-squares association criterion

- (GX) - Maximum inscribed association criterion

- (GN) - Minimum circumscribed association criterion

- (CC) - Circumference diameter (calculated size)

- (CA) - Area diameter (calculated size)

- (CV) - Volume diameter (calculated size)

- (SX) - Maximum size

- (SN) - Minimum size

- (SA) - Average size

- (SM) - Median size

- (SD) - Mid-range size

- (SR) - Range of sizes

- (E) - Envelope requirement

- ACS - Any cross section or sections

- SCS - Specific fixed cross section or sections