miim

### MP-042 Temperature Compensation hardware absent

The system is configured for Temperature Compensation, but the Temperature Compensation board is not present.

What you should do:

1. To clear the error, click Clear error in the XYZ Display window.

To clear it using an RCU-II, press and hold down the Servo Power Off button and then press the Joy button twice.

2. Obtain the necessary temperature compensation hardware.

3. If the error reoccurs, contact your Giddings & Lewis service representative.