cmm

#### Move Speed

Move Speed box

Use the Move Speed box to specify the move speed for the PH9 calibration. Depending on the state of the Display absolute speeds check box on the Part/Machine tab in the Setup Options dialog box, the Move Speed box and Touch Speed box can either accept an absolute speed (mm/sec) or a percentage of the machine's defined top speed.

For additional ways to affect the speed in the measurement process, see "Move Speed %" in the "Setting your Preferences" chapter of the PC-DMIS Core documentation.

The number in the Move Speed box can contain no more than four decimal places. If you enter a number with more than four decimal places, PC-DMIS rounds the number off at the fourth decimal place.