settingseditor

### DccPlnNumHits

Used to define the default value for the Hits per Row or the Hits per Ring values that will be used when a plane Auto Feature is created. Defines the number of hits to be used to measure the feature. The number of hits specified are equally spaced on the plane based on the pattern (whether using rows or rings). For more information, see "DccPlnPattern" and "DccPlnNumRows".

Entry Name: DccPlnNumHits

Entry Type: Whole number that specifies the number of permanent hits. The default value is 3.

See the "Working with Contact Path Properties" topic in the PC-DMIS CMM documentation.