Collapse All Expand All

PC-DMIS 2019 R1 Object Library |
Tip Object Members
See Also Overview Send Topic Feedback | See Object Hierarchy Chart

PCDLRN ActiveX DLL : Tip Object

Glossary Item Box

# Public Methods

ResetMeasToTheo | Resets measured tip data back to theo values

# Public Properties

a | Returns the A angle of the tip.
b | Returns the B angle of the tip.
C | Read Only: Returns the C angle of the tip
Date | Returns the PC-DMIS representation of the most recent calibration date of the tip.
diam | Returns the diameter of the tip.
DMISLabel | Read/Write: Gets/Sets the tip's DMIS Label
ID | Returns the ID string of the tip.
IJK | A PointData object that returns the vector along which the tip lies. Read-only.
MeasDiam | Read/Write: Gets/Sets the measured diameter of the tip
MeasThickness | Read Only: Returns the measured thickness of the the tip
MeasXYZ | Read/Write: Gets/Sets the measured XYZ data of the tip
Nickname | Read/Write: Gets/Sets the tip's nickname
Parent | Returns the Tips collection object that contains this tip.
PrbRdv | Read Only: Returns the PRBRDV value for an analog probe calibration
Selected | Determines whether tip is selected for qualification.
StandardDeviation | Read Only: Returns the standard deviation of the measured sphere after tip qualification
Thickness | Returns the nominal thickness of the tip.
Time | Returns the PC-DMIS representation of the most recent calibration time of the tip.
TipNum | Returns the tip number in the list of tips.
TipType | Returns the type of the tip.
WristOffset | Returns the wrist offset of the tip.
WristTipIJK | Returns the wrist tip vector of the tip.
XYZ | Returns the location of the tip.

# See Also

Tip Object

Copyright © 2019. Hexagon Manufacturing Intelligence – Metrology Software, Inc. All Rights Reserved.