laser

#### Cone Command Mode Text

CON1 =FEAT/LASER/CONE/DEFAULT,CARTESIAN,OUT

THEO/<3.1425,2.7539,0>,<0,0,1>,0.5,20,12.7

ACTL/<3.1425,2.7539,0>,<0,0,1>,0.5,20,12.7

TARG/<3.1425,2.7539,0>,<0,0,1>

DEPTH=0

CENTER OFFSET=3

SEARCH LENGTH=2

SHOW FEATURE PARAMETERS=YES

SURFACE=THEO_THICKNESS,0

RMEAS=NONE,NONE,NONE

AUTO WRIST=YES

GRAPHICAL ANALYSIS=NO

SHOW_LASER_PARAMETERS=YES

POINT CLOUD ID=COP1

SOUND=OFF

HORIZONTAL CLIPPING=0.0787,VERTICAL CLIPPING=0.0787

RINGBAND=ON,INNER OFFSET=0.5,OUTER OFFSET=2

OUTLIER_REMOVAL=ON,1

More:

Laser Cone

Cone Specific Parameters

Auto Cone Paths