core

#### To Create New Marked Sets

1. Select the Edit | Markings | New Marked Set option, or double-click anywhere in the Marked Sets window. The New Mark Set dialog box appears requesting a name for the new marked set.

New Mark Set dialog box

2. In Enter mark set label, type a name to identify the marked set. While there's no limit to the length of the name, short descriptive keywords improve readability.

3. Click OK. Your new marked set is stored in the Marked Sets window. At this point PC-DMIS also displays an Output Configuration dialog box. This dialog box allows you to define printing options specific to this marked set. (See "Setting Output and Printer Options for the Report Window" in "Using Basic File Options" for information on the various options in this dialog box.)

A sample Output Configuration dialog box for Set1

4. Define specific printing options for this set. Or, if you want to use the existing print options defined for your entire measurement routine, simply select the Use Global Print Settings check mark.

5. Click OK. The dialog box closes.

6. Now, you need to select this Marked Set and add features to it. To do this, follow the procedure in the "To Add or Remove Features on Existing Marked Sets" topic.