settingseditor

### DccTargIJK_2

Provides the default "K" value for various IJK vectors that are used in the creation of Auto Features using an NC-100 video probe. The value is applied to different vector types (Surface, Edge, etc.) depending on the auto feature type.

Because of the variance between auto features and how this value is applied, it is best to alter this value from the Auto Feature dialog box within PC-DMIS.

Entry Name: DccTargIJK_2

Entry Type: Real Number to specify the K vector value. The default value is 0.