Collapse All Expand All

PC-DMIS 2019 R1 Object Library |
Calibrate Method
See Also Send Topic Feedback | See Object Hierarchy Chart

sphere
  Id of measured sphere used in calibration.

tool
  Id of tool object used in calibration.

Moved
  Toggle indicating whether first hit should be taken manually or not. Can be either PCD_NO or PCD_YES.

PCDLRN ActiveX DLL > OldBasic Object : Calibrate Method

Glossary Item Box

# Description

Creates a probe calibration command

# Syntax

Visual Basic
    Public Sub Calibrate( _
       ByVal sphere As String, _
       ByVal tool As String, _
       ByVal Moved As PCDYESNO _
    )

# Parameters

sphere
  Id of measured sphere used in calibration.
tool
  Id of tool object used in calibration.
Moved

  Value | Description
  --- | ---
  PCD_NO |
  PCD_YES |

  Toggle indicating whether first hit should be taken manually or not. Can be either PCD_NO or PCD_YES.

# See Also

OldBasic Object | OldBasic Members

Copyright © 2019. Hexagon Manufacturing Intelligence – Metrology Software, Inc. All Rights Reserved.