settingseditor

### ColorMapValidateCadNormals

When this registry entry is set to True (1), PC-DMIS corrects CAD surface normals and makes them consistent when creating a FACE COLORMAP or POINT COLORMAP. For a solid, all normals are oriented outside of the material. For non-solid models, normals of adjacent faces are oriented in the same direction.

Entry Name: ColorMapValidateCadNormals

Entry Type: Whole Number that specifies True (1) or False (0). The default value is 0 (False).