miim

### MLB-095 Servo power failed to engage

The command to select automatic mode has been executed but the system was unable to turn on servo power.

As a result, the command is not executed.

What you should do:

1. Determine the cause of the problem.

Either correct the program or eliminate the hardware problem that is preventing servo power from engaging. Manually turn on servo power and select AUTO mode to continue the measurement routine.

2. If the error is supposed to support this operation:

   If the error reoccurs, contact your Giddings & Lewis service representative.