Collapse All Expand All

PC-DMIS 2019 R1 Object Library |
SetAutoVector Method
See Also Send Topic Feedback | See Object Hierarchy Chart

index
  Which vector to set.

I
  Double I value for the vector.

J
  Double J value for the vector.

K
  Double K value for the vector.

PCDLRN ActiveX DLL > OldBasic Object : SetAutoVector Method

Glossary Item Box

# Description

Sets Auto Vector Components (used inside StartFeature Block)

# Syntax

Visual Basic
    Public Sub SetAutoVector( _
       ByVal index As AUTOVECTORTYPES, _
       ByVal I As Double, _
       ByVal J As Double, _
       ByVal K As Double _
    )

# Parameters

index

  Value | Description
  --- | ---
  PCD_ANGLE_VECTOR |
  PCD_EDGE_REPORT_VECTOR |
  PCD_MEASURE_VECTOR |
  PCD_PIN_VECTOR |
  PCD_PUNCH_VECTOR |
  PCD_REPORT_VECTOR |
  PCD_SURF_REPORT_VECTOR |
  PCD_UPDATE_VECTOR |
  PCD_VECTOR1 |
  PCD_VECTOR2 |
  PCD_VECTOR3 |

  Which vector to set.
I
  Double I value for the vector.
J
  Double J value for the vector.
K
  Double K value for the vector.

# Remarks

This function is used for auto features only.

# See Also

OldBasic Object | OldBasic Members

Copyright © 2019. Hexagon Manufacturing Intelligence – Metrology Software, Inc. All Rights Reserved.