miim

### MP-046 Temperature Compensation or Digital I/O board failure

A read after write to digital outputs does not match actually written value. May also indicate a watchdog timer failure on the Temperature Compensation board.

What you should do:

1. To clear the error, click Clear error in the XYZ Display window.

To clear it using an RCU-II, press and hold down the Servo Power Off button and then press the Joy button twice.

2. If the error reoccurs, contact your Giddings & Lewis service representative.