laser

### Laser Probe Toolbox: Feature Extraction tab

Feature Extraction tab

You can use the Feature Extraction tab to specify ring band and feature-based clipping parameters as well as remove outliers on supported features.

The Feature Extraction tab is only available when using a laser sensor.

Depending on the feature type, the following feature extraction parameters are available:

- Feature Based Clipping parameters: This is available for all auto features.

- Ring Band parameters: This is only available for Circle, Cone, Cylinder, Round Slot, and Square Slot auto features.

- Filters:

- Remove outliers parameter: This is only available for Surface Point, Plane, Cone, Cylinder, Sphere, and Flush and Gap auto features.

- Remove points with normals outside parameter: This is only available for Surface Point, Plane, Circle, Round Slot, Square Slot, Polygon, Cylinder, Cone, and Sphere auto features.

Also see "Extracting Auto Features from Pointclouds".