miim

### MP-516 Front panel decode fail

A receiving or transmitting information error occurred at the front panel. The keypad entry returns to non-zero even though the entry is cleared. The cables to the front panel may not be connected properly.

For more information, see "MP Error Codes".

What you should do:

1. Make sure the cables to the front panel are connected properly.

2. If the error reoccurs, contact your Giddings & Lewis service representative.