nc

### CNC Select Table

Select Operation | CNC Programming | Select Table to open the CNC Select Table dialog box.

CNC Select Table dialog box

CNC/SELECTTABLE,TableNumber,CommandString

This command string is inserted inline in the generated NC measurement routine. It may be any text string, but should represent valid commands for the rotary table. No syntax checking is performed in PC-DMIS.

TableNumber Text string to specify the rotary table to which the command string will be sent.

CommandString Text string to be transferred to the rotary table for rotation.