Collapse All Expand All

PC-DMIS 2019 R1 Object Library |
Attach Object Members
See Also Overview Send Topic Feedback | See Object Hierarchy Chart

PCDLRN ActiveX DLL : Attach Object

Glossary Item Box

# Public Properties

AttachedAlign | ID associated with an alignment in the attached program that corresponds with an alignment in the attaching routine.
EXECUTE | This returns or sets a BOOLEAN value that determines whether or not the attached measurement routine should be executed when PC-DMIS encounters the attached routine.
ID | ID associated with the attached measurement routine. This ID identifies items in the attached measurement routine. For example, if the ID for the attach statement is "PART2", then feature "F1" in the attached routine can be referred to as "F1:PART2".
LocalAlign | ID associated with an alignment in the attaching program that corresponds to an alignment in the attached routine.
PartName | File name of the attached measurement routine.

# See Also

Attach Object

Copyright © 2019. Hexagon Manufacturing Intelligence – Metrology Software, Inc. All Rights Reserved.